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8-Port Gigabit Desktop Ethernet Switch
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Overview
    ADS108G 8-Port Gigabit desktop switch provides an easy way to make the transition to Gigabit Ethernet. All 8 ports support auto MDI/MDIX, no need to worry about the cable type, simply plug and play. Moreover, with the innovative energy-efficient technology, the ADS108G can save the power consumption, making it an eco-friendly solution for your business network.
  This new generation 8-Port Gigabit Desktop Switch ADS108G features the latest innovative energy-efficient technologies that can greatly expand your network capacity with much less power. It automatically adjusts power consumption according to the link status and cable length to limit the carbon footprint of your network. It also complies with the EU'S RoHS, prohibiting the use of certain hazardous materials. Besides, 80% of the packaging material can be recycled.
High Performance

  The ADS108G features non-blocking wire-speed architecture with a 16Gbps switching capacity for maximum data throughput. An 4K MAC address table provides scalability for even the largest networks. It also supports 802.3x Flow Control for full-duplex mode, and back pressure flow control for half-duplex mode alleviates traffic congestion and ensures reliable data transmission.

Ease to Use

 The auto features of this gigabit switch make installation plug and play and hassle-free. No configuring is required. Auto MDI/MDI-X crossover on all ports eliminate the need for crossover cables or uplink ports. Auto-negotiation on each port senses the link speed of a network device (either 10, 100 or 1000Mbps) and intelligently adjusts for compatibility and optimal performance. Compact size shell make it ideal for desktops with limited space while it is also convenient and safe. Dynamic LED lights provide real-time work status display. It features the latest innovative energy-efficient technologies that can greatly expand your network capacity with much less power. It automatically adjusts power consumption according to the link status and cable length to limit the carbon footprint of your network.

FEATURES

· 100% Data filtering rate eliminates all error packets
· Supports IEEE 802.3x flow control for Full Duplex mode and backpressure for Half Duplex mode
· Non-blocking switching architecture forwards and filters packets at full wire-speed for maximum throughput
· 16Gbps Switching Capacity
· Auto-MDI/MDIX eliminates the need for crossover cables
· Supports MAC address auto-learning and auto-aging
· Support the port N-Way Auto-Negotiation, Store and Forward
· Compact size design for desktops
· Plug and Play design simplifies installation
· Fanless design to make sure it works quietly
SPECIFICATIONS

	HARDWARE FEATURES

	Standards and Protocols
	IEEE 802.3i, IEEE 802.3u, IEEE 802.3ab, IEEE 802.3x, 802.1p

	Interface
	8 10/100/1000Mbps RJ45 Ports (Auto Negotiation/Auto MDI/MDIX)

	Network Media
	10BASE-T: UTP category 3, 4, 5 cable (maximum 100m)
100BASE-TX/1000BASE-T: UTP category 5, 5e or above cable (maximum 100m)

	Fan Quantity
	Fanless

	Power Supply
	100-240VAC, 50/60Hz input, 5vdc, 1A output

	Power Consumption
	Maximum: 4.08W (220V/50Hz)

	Dimensions ( W x D x H )
	 13*6.5*2.7cm


	PERFORMANCE

	Switching Capacity
	16Gbps

	Packet Forwarding Rate
	11.9Mpps

	MAC Address Table
	4K

	Transfer Method
	Store-and-Forward


	SOFTWARE FEATURES

	Advanced Features
	MAC address auto-learning and auto-aging
IEEE802.3x Flow control


	Certification
	FCC, CE, RoHS

	Package Contents
	8-Port Gigabit Desktop Switch
Power adapter

	Environment
	Operating Temperature: 0℃~40℃ (32℉~104℉);
Storage Temperature: -40℃~70℃ (-40℉~158℉);
Operating Humidity: 10%~90% non-condensing;
Storage Humidity: 5%~90% non-condensing
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